# CLS

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
CLS [colour]

Description:
Clears the VGA screen and the terminal emulator's screen.

On all devices except DOS and mono Maximite, optionally 'colour' can be specified which will be used for the VGA background when clearing the screen.

cls rgb(red)

Last edited: 29 September, 2020