# PAUSE

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
PAUSE delay-mS

Description:
Halt execution of the running program for ‘delay’ ms. This can be a fraction.
For example, 0.2 is equal to 200 ěs. The maximum delay is 2147483647 ms (about 24 days).
Note that interrupts will be recognised and processed during a pause.

Last edited: 30 September, 2020