# PLAY TTS

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
PLAY TTS [PHONETIC] text [,speed] [,pitch] [,mouth] [,throat] [, interrupt]

Description:
Outputs text as speech on the DAC outputs.
See http://www.retrobits.net/atari/sam.shtml for details of parameter usage.
The command is non-blocking and the speech is played in the background. 'interrupt' is optional and is the name of a subroutine which will be called when the speech has finished playing.

Last edited: 15 December, 2020