# New Connection

MMEdit can connect to your device by serial or TCP/IP

Selecting 'new' from the 'connect' menu will open a dialog that allows you to enter a TCP/IP address an dprot number if using TCP/IP

For serial ports, either set the port number and baud rate or select 'find ports' to list all available serial ports currently on your computer.
you can also adjust the delay inserted in lines sent during 'autoisave' etc and a different delay when in the Maximite's editor.

If you have any serial pots that you don't want listed in the available ports list, enter them in the 'Excluded serial ports' text field

The last 10 connections are remembered but can be cleared if desired.

Last edited: 02 November, 2020