# LINE

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
LINE x1, y1, x2, y2 [, LW [, C]]
LINE [(x1 , y1)] - (x2, y2) [,c [,B[F]]]

Description:

LINE x1, y1, x2, y2 [, LW [, C]] (not CMM V1 or mono Maximite)
Draws a line starting at the coordinates ‘x1’ and ‘y1’ and ending at ‘x2’ and ‘y2’. ‘LW’ is the line’s width and is only valid for horizontal or vertical lines.
It defaults to 1 if not specified or if the line is a diagonal. ‘C’ is an integer representing the colour and defaults to the current foreground colour.
All parameters can now be expressed as arrays and the software will plot the number of lines as determined by the dimensions of the smallest array.
'x1', 'y1', 'x2', and 'y2' must all be arrays or all be single variables /constants otherwise an error will be generated. 'lw' and 'c' can be either arrays or single variables/constants.

LINE [(x1 , y1)] - (x2, y2) [,c [,B[F]]] (CMM V1 and Mono Maximite)
Draws a line or box on the video screen. x1,y1 and x2,y2 specify the beginning and end points of a line. 'c' specifies the colour and defaults to the default foreground colour if not specified.
It can also be -1 to invert the pixels. (x1, y1) is optional and if omitted the last drawing point will be used.
The optional B will draw a box with the points (x1,y1) and (x2,y2) at opposite corners. The optional BF will draw a box (as ,B) and fill the interior.
This mode can be used on the CMM2 if OPTION LEGACY is set

Also see LINE INPUT

Last edited: 30 September, 2020