# CLOSE

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
CLOSE [#]nbr [,[#]nbr] ...

Description:
Close the file(s) previously opened with the file number ‘#fnbr’

Close the serial communications port(s) previously opened with the file number ‘nbr’.
The # is optional. Also see the OPEN command.

The text “GPS” can be substituted for [#]nbr to close a communications port
used for a GPS receiver (for those devices that support GPS)

Not all files are closed automatically when the program ends so it is good practice to CLOSE them before exiting.

Last edited: 29 September, 2020