# UPDATE FIRMWARE

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
UPDATE FIRMWARE

Description:
Switch the STM32 CPU into firmware update mode.
This is the same as switching the BOOT CONFIG switch on the Waveshare CPU board to SYSTEM and allows for quick firmware updates without opening the Maximite's case.
You should cycle the power following a firmware update or if this command was accidently used.
This will return the STM32 CPU to normal mode.

Last edited: 29 September, 2020