# CPU RESTART

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
CPU RESTART

Description:
Will force a restart of the processor.
This will clear all variables and reset everything (eg, timers, COM ports, I2C,
etc) similar to a power up situation but without the power up banner.
If OPTION AUTORUN has been set the program will restart.

Also see CPU speed and CPU SLEEP

Last edited: 28 January, 2021