# SEEK

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
SEEK [#]fnbr, pos

Description:
Will position the read/write pointer in a file that has been opened on the SD card for RANDOM access to the 'pos' byte.
The first byte in a file is numbered one so SEEK #5,1 will position the read/write pointer to the start of the file.

Last edited: 30 September, 2020