# FONT

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
FONT [#]font-number, scaling

Description:
This will set the default font for displaying text on the VGA screen. Fonts are specified as a number.
For example, #2 (the # is optional)
'scaling' can range from 1 to 15 and will multiply the size of the pixels making the displayed character correspondingly wider and higher.
Eg, a scale of 2 will double the height and width.

Also see LOAD FONT and FONT LOAD

Last edited: 29 September, 2020