This is a list of known bugs and issues in PicoMite MMBasic 5.07.07.  
These should be fixed in later versions.

==================================================================================

MM.INFO(OPTION ANGLE) returns an incorrect value. Fixed in V5.07.08b5
FORMAT$ function may not yield expected results (WebMite only). Waiting on fix from Pi foundation
Web functionality may not work with CPU speeds below 126MHz. Speed limited to 126MHz in V5.07.08b5
Minor bugs in CALL and MM.CMDLINE$. Fixed in V5.07.08b5
LOAD SPRITE requires exact spacing of the width,numer,height fields. Fixed in V5.07.08b5.
Changing volume when PLAY TONE is playing the same on both channels causes one channel to disappear. Fixed in V5.07.08b5.
A TCP request while in the editor causes the WebMite to crash. Fixed in V5.07.08b5.
Memory leak in WEB MQTT PUBLISH. Fixed in V5.07.08b5.
EXECUTE command does not work at the command prompt. Fixed in V5.07.08b5.
CLS after NEW when a framebuffer is active can crash system. Fixed in V5.07.08b5.
Using EXECUTE in a program that has been AUTORUN crashes the system. Fixed in V5.07.08b5.
Bug in FRAMEBUFFER COPY to N. Fixed in V5.07.08b7
Bug in FRAMEBUFFER CLOSE. Fixed in V5.07.08b7
Race condition when PLAY TONE is used with defined time and a new tone is issued during the termination. Fixed in V5.07.08b8
Bug in PIN(TEMP) after another adc channel is used - Fixed in V5.07.08b12
Bug in reading a single adc channel after the ADC command is used  - Fixed in V5.07.08b12


