V5.09.00b0

Introduction of USB variants for PicoMite and PicoMiteVGA
Rationalisation of BLIT and SPRITE
PRINT to a VGA screen or console LCD now respects OPTION TAB (defaults to 2)

V5.09.00b1

OPTION SDCARD COMBINED CS 'saves a pin by sharing the touch CS pin with the SDcard
OPTION LCDPANEL SSD1963_N_16, orientation [,backlightpin] [,DCpin] [,NORESET]
OPTION LCDPANEL ILI9341_16, orientation [,backlightpin] [,DCpin] [,NORESET]
OPTION LCDPANEL IPS_4_16, orientation [,backlightpin] [,DCpin] [,NORESET]
OPTION LCDPANEL ILI9341_8, orientation [,backlightpin] [,DCpin] [,NORESET]
OPTION LCDPANEL SSD1963_N_8, orientation [,backlightpin] [,DCpin] [,NORESET]

Fixes bug in reading from 8-bit SSD 1963 displays