# MEMORY

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
MEMORY

Description:
List the amount of memory currently in use. For example, on the CMM2:
Flash:
39K ( 6%) Program (1450 lines)
527K (94%) Free
RAM:
0K ( 0%) 0 Variables
1K ( 0%) General
5470K (100%) Free
Notes:
General memory is used by serial I/O buffers, etc.
Memory usage is rounded to the nearest 1K byte.

Last edited: 30 September, 2020