# PLAY

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
PLAY NEXT
PLAY PREVIOUS
PLAY PAUSE
PLAY PAUSE
PLAY STOP
PLAY VOLUME left, right

Description:

PLAY PAUSE will temporarily halt the currently playing file or tone.

PLAY RESUME will resume playing a sound that was paused.

PLAY STOP will terminate the playing of the file or tone. When the program terminates for whatever reason the sound output will also be automatically stopped.

PLAY NEXT
PLAY PREVIOUS
When playing a sequence of audio tracks (by using PLAY MP3 on a directory holding multiple MP3 files) these commands can be used to skip forward or back a file.
The commands PLAY PAUSE, RESUME, VOLUME
can also be used.

PLAY VOLUME left, right
Will adjust the volume of the audio output.
'left' and 'right' are the levels to use for the left and right channels and can be between 0 and 100 with 100 being the maximum volume.
There is a linear relationship between the specified level and the output. The volume defaults to maximum when a program is run.

PLAY VOLUME does not have any effect on PLAY SOUND output.

Last edited: 29 September, 2020