# HELP

Compatible with:
DOS Maximite CMM MM150 MM170 MM+ MMX Picromite ArmiteL4 Armite F4 ArmiteH7 Picomite CMM2

Syntax:
HELP [text]

Description:

This displays up to 3 lines of help that match the "text". text isn't quoted.
If text isn't specified you can type characters into the help command and the display will show up to three lines than match.
Use the delete key to remove characters
You can use up arrow and down arrow to move through matches (e.g. for things like MM.INFO)

Exit the help command with either ESC or F12
The intention of the facility is just to provide a quick check on command syntax and will never replace this written manual.
The command can be called from within the editor using F12. In this case the HELP command is called with any characters surrounding the cursor that can form part of a command or function name. So if the cursor is positioned on the 'I' of a DIM command the help will immediately show the syntax for DIM

Last edited: 15 December, 2020